 (
Roof with overhang secured with 4 screws only for inspection if necessary.
)The Northumberland Kestrel box - 2015
 (
1
3
cm
) (
Hanmer 201
5
) (
Screw lid down at front corners. Make sure you can remove the screws!
) (
H
ole
 size
 -   
13c
m diameter hole for 
Kestrel
) (
Roof with overhang secured with 4 
s
crews only for inspection if necessary.
) (
Front 
 (
x1)
) (
32
cm
) (
30
cm
) (
Back (x1)
) (
32cm
) (
30cm
) (
6
0cm
) (
30
cm
) (
Hanmer 201
5
) (
3
0
cm
) (
5
0cm
) (
Roof (X1)
) (
Base & Sides
 (X
3
)
) (
Use a minimum wood thickness of 18mm (exterior quality ply)
Paint the whole exterior first with water based fence paint; then paint over the roof with an oil based outside gloss.
) (
Plan view inside box.
) (
Bolt the box 
to a 
6
5cm batten and attach 
this to a
 tree
 or side of a barn
. (
4
 metres is high enough) 
)
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