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Attach the box to a 48cm wooden batten
)







 (
Use a minimum wood thickness of 18mm (exterior quality)
Paint the whole exterior first with water based fence paint; then paint over the roof with an oil based outside gloss.
)
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