
The Northumberland Top Opening Bird Box-
For Sparrows, Tits & Redstarts
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Screw on to a 40cm batten and attach to the tree
. 1 to 2 metres is high enough for the birds; only place higher if human interference is likely.
)






 (
The top (1
6
cm by 1
6
cm) should overhang at the front and sides 
Roof hinge made from tape or roofing flashing.
Screw lid down at front corners. Make sure you can remove the screws.
)
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Paint the roof and base only. 
First with water based fence paint; then the roof can be painted with outside gloss
 
paint
. 
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Use plank wood (treated or untreated) approximately 2cm thickness. 
The front, back and top 15cm wide planks.
The sides and bottom 10cm wide planks.
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Use 
(
plank
)
 wood
 for sides, front, back and base
 (treated or untreated) approximately 2cm thickness. 
Front, base and back 10cm wide planks.
Sides 1
5
cm wide planks 
Top 1
6
cm
.
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Plan view inside box.
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Plan view inside box.
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Plan view inside box.
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Hole
 size 
 40mm diameter hole for Redstarts
 28
mm for 
Tree Sparrows & Great Tits
 25mm for small Tits
)
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Insert base 
slightly
 up from the bottom of the box. 
Trim base by a few millimetres to fit it in to the bottom of the box.
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